% ----------------------------------------------------------------------------
%
% Changes:    <By whom>, <When>, <What changes> 
% 
%      H. Wabnig, 1.3.'93, created
%
%  NOTE: This is no independent LaTex file. It has to be included in the
%        file that describes the corresponding ACPC group
%        or in a `frame' LaTex file (see `hw-frame.tex') where
%        formating information etc is given.
%
% ----------------------------------------------------------------------------

\subsection{MultiCluster-3DE}

\subsubsection{Footprint}

\begin{center}
\begin{tabular}{|c|l|}\hline
System               & MC-3DE (Local Development Station)	\\ \hline
Architecture         & Distributed Memory MIMD         		\\ \hline
\# of Processors     & 16                               	\\ \hline
Type of Processors   & T800 				     	\\ \hline
Memory Size          & 16$\times$4 MB = 64 MB          		\\ \hline
Disk Capacity        & 0 MB			       		\\ \hline
Operating System     & Parix Release 1.1 	         	\\ \hline  \hline
Name                 & ---				 	\\ \hline
Internet Address     & ---	                 		\\ \hline
Location             & Lenaugasse 2/8 1080 Vienna        	\\ \hline
System Administrator & H.\ Wabnig (wabnig)       		\\ \hline
Network Coordinator  & H.\ Wabnig (wabnig)			\\ \hline
\end{tabular}
\end{center}


\subsubsection{Availability}

\begin{center}
\begin{tabular}{|c|c|c|c|c|c|c|c|}\hline
Group       & RISC & TU-Vienna & Vienna & Linz & Salzburg & World \\ \hline
            & slow & good      & good   &      & slow     & good \\ \hline
\end{tabular}
\end{center}


\subsubsection{Further Description}

Our transputer system is a local development station. Although the parix concept 
contains software for multiuser administration it is not applicable to the MC-3DE
hardware. Therefore these software parts are not included and multiuser processing
is not possible. Nevertheless the system can be used over the network. But the 
system administrator has to be contacted to set up the system accordingly and 
prevent problems caused by multiple users. 

The MC-3DE has a fixed topology (mesh). Special topology configurations can be 
built with cables. \\

{\bf Footprint of the Host Computer}

\begin{center}
\begin{tabular}{|c|l|}\hline
System               & SUN IPX  				\\ \hline
Type of Processors   & Sparc					\\ \hline
Memory Size          & 32 MByte            			\\ \hline
Disk Capacity        & 1.2 GByte               			\\ \hline
Operating System     & SunOS Release 4.1.1-IPX         		\\ \hline  \hline
Name                 & epikur.ani.univie.ac.at  		\\ \hline
Internet Address     & 131.130.32.113     			\\ \hline
Location             & Lenaugasse 2/8 1080 Vienna     		\\ \hline
System Administrator & U.\ Presslauer (ursula)			\\ \hline
Network Coordinator  & U.\ Presslauer (ursula)			\\ \hline
\end{tabular}
\end{center}


\subsubsection{Software}

